# S.M.A.R.T. Input Plugin

Get metrics using the command line utility `smartctl` for S.M.A.R.T. (Self-Monitoring, Analysis and Reporting Technology) storage devices. SMART is a monitoring system included in computer hard disk drives (HDDs) and solid-state drives (SSDs) that detects and reports on various indicators of drive reliability, with the intent of enabling the anticipation of hardware failures.
See smartmontools (<https://www.smartmontools.org/>).

SMART information is separated between different measurements: `smart_device` is used for general information, while `smart_attribute` stores the detailed attribute information if `attributes = true` is enabled in the plugin configuration.

If no devices are specified, the plugin will scan for SMART devices via the following command:

```sh
smartctl --scan
```

Metrics will be reported from the following `smartctl` command:

```sh
smartctl --info --attributes --health -n <nocheck> --format=brief <device>
```

This plugin supports _smartmontools_ version 5.41 and above, but v. 5.41 and v. 5.42
might require setting `nocheck`, see the comment in the sample configuration.
Also, NVMe capabilities were introduced in version 6.5.

To enable SMART on a storage device run:

```sh
smartctl -s on <device>
```

## NVMe vendor specific attributes

For NVMe disk type, plugin can use command line utility `nvme-cli`. It has a feature
to easy access a vendor specific attributes.
This plugin supports nmve-cli version 1.5 and above (<https://github.com/linux-nvme/nvme-cli>).
In case of `nvme-cli` absence NVMe vendor specific metrics will not be obtained.

Vendor specific SMART metrics for NVMe disks may be reported from the following `nvme` command:

```sh
nvme <vendor> smart-log-add <device>
```

Note that vendor plugins for `nvme-cli` could require different naming convention and report format.

To see installed plugin extensions, depended on the nvme-cli version, look at the bottom of:

```sh
nvme help
```

To gather disk vendor id (vid) `id-ctrl` could be used:

```sh
nvme id-ctrl <device>
```

Association between a vid and company can be found there: <https://pcisig.com/membership/member-companies>.

Devices affiliation to being NVMe or non NVMe will be determined thanks to:

```sh
smartctl --scan
```

and:

```sh
smartctl --scan -d nvme
```

## Configuration

```toml
# Read metrics from storage devices supporting S.M.A.R.T.
[[inputs.smart]]
    ## Optionally specify the path to the smartctl executable
    # path_smartctl = "/usr/bin/smartctl"
  
    ## Optionally specify the path to the nvme-cli executable
    # path_nvme = "/usr/bin/nvme"
  
    ## Optionally specify if vendor specific attributes should be propagated for NVMe disk case
    ## ["auto-on"] - automatically find and enable additional vendor specific disk info
    ## ["vendor1", "vendor2", ...] - e.g. "Intel" enable additional Intel specific disk info
    # enable_extensions = ["auto-on"]
  
    ## On most platforms used cli utilities requires root access.
    ## Setting 'use_sudo' to true will make use of sudo to run smartctl or nvme-cli.
    ## Sudo must be configured to allow the telegraf user to run smartctl or nvme-cli
    ## without a password.
    # use_sudo = false
  
    ## Skip checking disks in this power mode. Defaults to
    ## "standby" to not wake up disks that have stopped rotating.
    ## See --nocheck in the man pages for smartctl.
    ## smartctl version 5.41 and 5.42 have faulty detection of
    ## power mode and might require changing this value to
    ## "never" depending on your disks.
    # nocheck = "standby"
  
    ## Gather all returned S.M.A.R.T. attribute metrics and the detailed
    ## information from each drive into the 'smart_attribute' measurement.
    # attributes = false
  
    ## Optionally specify devices to exclude from reporting if disks auto-discovery is performed.
    # excludes = [ "/dev/pass6" ]
  
    ## Optionally specify devices and device type, if unset
    ## a scan (smartctl --scan and smartctl --scan -d nvme) for S.M.A.R.T. devices will be done
    ## and all found will be included except for the excluded in excludes.
    # devices = [ "/dev/ada0 -d atacam", "/dev/nvme0"]
  
    ## Timeout for the cli command to complete.
    # timeout = "30s"
```

## Permissions

It's important to note that this plugin references smartctl and nvme-cli, which may require additional permissions to execute successfully.
Depending on the user/group permissions of the telegraf user executing this plugin, you may need to use sudo.

You will need the following in your telegraf config:

```toml
[[inputs.smart]]
  use_sudo = true
```

You will also need to update your sudoers file:

```bash
$ visudo
# For smartctl add the following lines:
Cmnd_Alias SMARTCTL = /usr/bin/smartctl
telegraf  ALL=(ALL) NOPASSWD: SMARTCTL
Defaults!SMARTCTL !logfile, !syslog, !pam_session

# For nvme-cli add the following lines:
Cmnd_Alias NVME = /path/to/nvme
telegraf  ALL=(ALL) NOPASSWD: NVME
Defaults!NVME !logfile, !syslog, !pam_session
```

To run smartctl or nvme with `sudo` wrapper script can be created. `path_smartctl` or
`path_nvme` in the configuration should be set to execute this script.

## Metrics

- smart_device:
  - tags:
    - capacity
    - device
    - enabled
    - model
    - serial_no
    - wwn
  - fields:
    - exit_status
    - health_ok
    - read_error_rate
    - seek_error
    - temp_c
    - udma_crc_errors

- smart_attribute:
  - tags:
    - capacity
    - device
    - enabled
    - fail
    - flags
    - id
    - model
    - name
    - serial_no
    - wwn
  - fields:
    - exit_status
    - raw_value
    - threshold
    - value
    - worst

### Flags

The interpretation of the tag `flags` is:

- `K` auto-keep
- `C` event count
- `R` error rate
- `S` speed/performance
- `O` updated online
- `P` prefailure warning

### Exit Status

The `exit_status` field captures the exit status of the used cli utilities command which
is defined by a bitmask. For the interpretation of the bitmask see the man page for
smartctl or nvme-cli.

## Device Names

Device names, e.g., `/dev/sda`, are *not persistent*, and may be
subject to change across reboots or system changes. Instead, you can use the
*World Wide Name* (WWN) or serial number to identify devices. On Linux block
devices can be referenced by the WWN in the following location:
`/dev/disk/by-id/`.

## Troubleshooting

If you expect to see more SMART metrics than this plugin shows, be sure to use a proper version
of smartctl or nvme-cli utility which has the functionality to gather desired data. Also, check
your device capability because not every SMART metrics are mandatory.
For example the number of temperature sensors depends on the device specification.

If this plugin is not working as expected for your SMART enabled device,
please run these commands and include the output in a bug report:

For non NVMe devices (from smartctl version >= 7.0 this will also return NVMe devices by default):

```sh
smartctl --scan
```

For NVMe devices:

```sh
smartctl --scan -d nvme
```

Run the following command replacing your configuration setting for NOCHECK and
the DEVICE (name of the device could be taken from the previous command):

```sh
smartctl --info --health --attributes --tolerance=verypermissive --nocheck NOCHECK --format=brief -d DEVICE
```

If you try to gather vendor specific metrics, please provide this commad
and replace vendor and device to match your case:

```sh
nvme VENDOR smart-log-add DEVICE
```

## Example SMART Plugin Outputs

```shell
smart_device,enabled=Enabled,host=mbpro.local,device=rdisk0,model=APPLE\ SSD\ SM0512F,serial_no=S1K5NYCD964433,wwn=5002538655584d30,capacity=500277790720 udma_crc_errors=0i,exit_status=0i,health_ok=true,read_error_rate=0i,temp_c=40i 1502536854000000000
smart_attribute,capacity=500277790720,device=rdisk0,enabled=Enabled,fail=-,flags=-O-RC-,host=mbpro.local,id=199,model=APPLE\ SSD\ SM0512F,name=UDMA_CRC_Error_Count,serial_no=S1K5NYCD964433,wwn=5002538655584d30 exit_status=0i,raw_value=0i,threshold=0i,value=200i,worst=200i 1502536854000000000
smart_attribute,capacity=500277790720,device=rdisk0,enabled=Enabled,fail=-,flags=-O---K,host=mbpro.local,id=199,model=APPLE\ SSD\ SM0512F,name=Unknown_SSD_Attribute,serial_no=S1K5NYCD964433,wwn=5002538655584d30 exit_status=0i,raw_value=0i,threshold=0i,value=100i,worst=100i 1502536854000000000
```
