# Iptables Input Plugin

The iptables plugin gathers packets and bytes counters for rules within a set
of table and chain from the Linux's iptables firewall.

Rules are identified through associated comment. **Rules without comment are
ignored**.  Indeed we need a unique ID for the rule and the rule number is not
a constant: it may vary when rules are inserted/deleted at start-up or by
automatic tools (interactive firewalls, fail2ban, ...).  Also when the rule set
is becoming big (hundreds of lines) most people are interested in monitoring
only a small part of the rule set.

Before using this plugin **you must ensure that the rules you want to monitor
are named with a unique comment**. Comments are added using the `-m comment
--comment "my comment"` iptables options.

The iptables command requires CAP_NET_ADMIN and CAP_NET_RAW capabilities. You
have several options to grant telegraf to run iptables:

* Run telegraf as root. This is strongly discouraged.
* Configure systemd to run telegraf with CAP_NET_ADMIN and CAP_NET_RAW. This is
  the simplest and recommended option.
* Configure sudo to grant telegraf to run iptables. This is the most
  restrictive option, but require sudo setup.

## Using systemd capabilities

You may run `systemctl edit telegraf.service` and add the following:

```shell
[Service]
CapabilityBoundingSet=CAP_NET_RAW CAP_NET_ADMIN
AmbientCapabilities=CAP_NET_RAW CAP_NET_ADMIN
```

Since telegraf will fork a process to run iptables, `AmbientCapabilities` is
required to transmit the capabilities bounding set to the forked process.

## Using sudo

You will need the following in your telegraf config:

```toml
[[inputs.iptables]]
  use_sudo = true
```

You will also need to update your sudoers file:

```bash
$ visudo
# Add the following line:
Cmnd_Alias IPTABLESSHOW = /usr/bin/iptables -nvL *
telegraf  ALL=(root) NOPASSWD: IPTABLESSHOW
Defaults!IPTABLESSHOW !logfile, !syslog, !pam_session
```

## Using IPtables lock feature

Defining multiple instances of this plugin in telegraf.conf can lead to
concurrent IPtables access resulting in "ERROR in input [inputs.iptables]: exit
status 4" messages in telegraf.log and missing metrics. Setting 'use_lock =
true' in the plugin configuration will run IPtables with the '-w' switch,
allowing a lock usage to prevent this error.

## Global configuration options <!-- @/docs/includes/plugin_config.md -->

In addition to the plugin-specific configuration settings, plugins support
additional global and plugin configuration settings. These settings are used to
modify metrics, tags, and field or create aliases and configure ordering, etc.
See the [CONFIGURATION.md][CONFIGURATION.md] for more details.

[CONFIGURATION.md]: ../../../docs/CONFIGURATION.md

## Configuration

```toml @sample.conf
# Gather packets and bytes throughput from iptables
[[inputs.iptables]]
  ## iptables require root access on most systems.
  ## Setting 'use_sudo' to true will make use of sudo to run iptables.
  ## Users must configure sudo to allow telegraf user to run iptables with
  ## no password.
  ## iptables can be restricted to only list command "iptables -nvL".
  use_sudo = false
  ## Setting 'use_lock' to true runs iptables with the "-w" option.
  ## Adjust your sudo settings appropriately if using this option
  ## ("iptables -w 5 -nvl")
  use_lock = false
  ## Define an alternate executable, such as "ip6tables". Default is "iptables".
  # binary = "ip6tables"
  ## defines the table to monitor:
  table = "filter"
  ## defines the chains to monitor.
  ## NOTE: iptables rules without a comment will not be monitored.
  ## Read the plugin documentation for more information.
  chains = [ "INPUT" ]
```

## Measurements & Fields

* iptables
  * pkts (integer, count)
  * bytes (integer, bytes)

## Tags

* All measurements have the following tags:
  * table
  * chain
  * ruleid

The `ruleid` is the comment associated to the rule.

## Example Output

```text
$ iptables -nvL INPUT
Chain INPUT (policy DROP 0 packets, 0 bytes)
pkts bytes target     prot opt in     out     source               destination
100   1024   ACCEPT     tcp  --  *      *       192.168.0.0/24       0.0.0.0/0            tcp dpt:22 /* ssh */
 42   2048   ACCEPT     tcp  --  *      *       192.168.0.0/24       0.0.0.0/0            tcp dpt:80 /* httpd */
```

```shell
$ ./telegraf --config telegraf.conf --input-filter iptables --test
iptables,table=filter,chain=INPUT,ruleid=ssh pkts=100i,bytes=1024i 1453831884664956455
iptables,table=filter,chain=INPUT,ruleid=httpd pkts=42i,bytes=2048i 1453831884664956455
```
